{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["history","GF3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"history","index":0,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[[5,1,7,1]],"flags":["formulas_cached_only"]}
[]
[null,"DMC-GF3"]
[null,null,null,"Original","Revised"]
[null,"2011-06-06","Weight","Approx. 267g / 9.42 oz    （SD card, Battery, Body)\nApprox. 322g / 11.36 oz  （SD card, Battery, H-H014 lens included） \nApprox. 432g / 15.24 oz   (SD card, Battery, H-FS014042 lens included)","Approx. 264g / 9.31 oz    （SD card, Battery, Body)\nApprox. 319g / 11.25 oz  （SD card, Battery, H-H014 lens included） \nApprox. 429g / 15.13 oz   (SD card, Battery, H-FS014042 lens included)"]
[null,"2011-06-07","Microphone","Stereo, Wind-cut: Off / Low / Standard / High\nMicrophone level adjustable: Lv1 / Lv2 / Lv3 / Lv4","Monaural, Wind-cut: Off / Low / Standard / High\nMicrophone level adjustable: Lv1 / Lv2 / Lv3 / Lv4"]
[null,"2011-06-08","Continuous recordable time (Motion images)","AVCHD with picture quality set to [SH]: Approx. 160 min with H-FS014042 / Approx. 170 min with H-H014","AVCHD with picture quality set to [FSH]: Approx. 160 min with H-FS014042 / Approx. 170 min with H-H014"]
[null,null,"Actual recordable time (Motion images)","AVCHD with picture quality set to [SH]: Approx. 130 min with H-FS014042 / Approx. 150 min with H-H014","AVCHD with picture quality set to [FSH]: Approx. 130 min with H-FS014042 / Approx. 150 min with H-H014"]
[null,null,"Weight","Approx. 225g / 7.94 oz    （Body only)","Approx. 222g / 7.83 oz    （Body only)"]

{"sheet":"GF3","index":1,"n_rows":95,"n_cols":7,"rows_kept":95,"cut":false,"hidden":false,"merged":[[11,0,27,0],[35,0,42,0],[56,0,60,0],[87,6,87,12],[69,6,69,7],[26,1,26,4],[80,1,80,4],[72,1,72,4],[73,1,73,4],[74,1,74,4],[71,1,71,4],[62,1,62,4],[27,1,27,4],[66,0,69,0],[66,1,66,4],[67,1,67,4],[68,1,69,4],[61,0,65,0],[61,1,61,4],[56,1,56,4],[88,1,90,4],[91,1,92,4],[88,0,92,0],[84,0,85,0],[84,1,84,4],[85,1,85,4],[86,0,87,0],[86,1,86,4],[87,1,87,4],[81,0,83,0],[81,1,82,4],[83,1,83,4],[76,1,76,4],[77,1,77,4],[75,0,79,0],[78,1,78,4],[79,1,79,4],[75,1,75,4],[63,1,63,4],[64,1,64,4],[65,1,65,4],[70,1,70,4],[60,1,60,4],[50,0,51,0],[50,1,50,4],[51,1,51,4],[52,0,55,0],[52,1,52,4],[53,1,55,4],[57,1,58,4],[48,1,48,4],[49,1,49,4],[47,0,49,0],[59,1,59,4],[45,1,45,4],[41,1,41,4],[40,1,40,4],[47,1,47,4],[35,1,35,4],[42,1,42,4],[43,1,43,4],[44,1,44,4],[16,1,25,1],[21,2,25,2],[22,3,25,3],[22,4,23,4],[24,4,25,4],[34,1,34,4],[2,0,5,0],[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,1,5,4],[13,1,13,4],[14,1,14,4],[20,3,21,4],[16,2,19,4],[11,1,12,4],[72,0,73,0],[28,0,34,0],[28,1,28,4],[29,1,29,4],[36,1,36,4],[37,1,37,4],[38,1,38,4],[30,1,30,4],[31,1,31,4],[43,0,46,0],[32,1,32,4],[33,1,33,4],[6,0,10,0],[6,1,6,4],[15,1,15,4],[7,1,7,4],[8,1,8,4],[9,1,9,4],[10,1,10,4]],"flags":["formulas_cached_only"]}
[{"$nulls":5},"Ver.","2010-10-21"]
["DMC-GF3 Specifications"]
["TYPE","Type",null,null,null,"Digital interchangeable lens system camera"]
[null,"Recording media",null,null,null,"SD memory card, SDHC memory card,  SDXC memory card "]
[null,"Image sensor size",null,null,null,"17.3 x 13.0 mm (in 4:3 aspect ratio)"]
[null,"Lens mount",null,null,null,"Micro Four Thirds mount"]
["IMAGE SENSOR","Type",null,null,null,"Live MOS Sensor"]
[null,"Total pixels",null,null,null,"13.06 Megapixels"]
[null,"Camera effective pixels",null,null,null,"12.10 Megapixels"]
[null,"Color filter",null,null,null,"Primary color filter"]
[null,"Dust reduction system",null,null,null,"Supersonic wave filter"]
["RECORDING SYSTEM","Recording file format",null,null,null,"Still Image: JPEG(DCF, Exif 2.3), RAW,\nMPO (When attaching 3D lens in Micro Four Thirds standard)"]
[{"$nulls":5},"Motion Image: AVCHD / QuickTime Motion JPEG"]
[null,"Aspect ratio",null,null,null,"4:3, 3:2, 16:9, 1:1"]
[null,"Image quality",null,null,null,"RAW, RAW+Fine, RAW+Standard, Fine, Standard, \nMPO+Fine, MPO+Standard (with 3D lens in Micro Four Thirds System standard)"]
[null,"Color space",null,null,null,"sRGB, Adobe RGB"]
[null,"File size(Pixels) ","Still Image",null,null,"[4:3] 4000x3000(L) / 2816x2112(M) / 2048x1536(S) / 1600x1200(When attaching 3D lens in Micro Four Third System standard)"]
[{"$nulls":5},"[3:2] 4000x2672(L) / 2816x1880(M) / 2048x1360(S) / 1600x1064(When attaching 3D lens in Micro Four Third System standard)"]
[{"$nulls":5},"[16:9] 4000x2248(L) / 2816x1584(M) / 1920x1080(S) / 1600x904(When attaching 3D lens in Micro Four Third System standard)"]
[{"$nulls":5},"[1:1] 2992 x 2992 (L) / 2112 x 2112 (M) / 1504 x 1504 (S) / 1440x1440(When attaching 3D lens in Micro Four Third System standard)"]
[null,null,"Motion Image","Motion JPEG*1",null,"[4:3] QVGA : 320 x 240, 30fps / VGA : 640 x 480, 30fps"]
[{"$nulls":5},"[HD] 1280 x 720, 30fps"]
[null,null,null,"AVCHD*2","NTSC","[Full HD] 1920×1080, 60i (sensor output is 30p) (FSH:17Mbps)"]
[{"$nulls":5},"[HD] 1280 x 720, 60p (sensor output is 30p)（SH:17Mbps)"]
[{"$nulls":4},"PAL","[Full HD] 1920×1080, 50i (sensor output is 25p) (FSH:17Mbps)"]
[{"$nulls":5},"[HD] 1280 x 720, 50p (sensor output is 25p)（SH:17Mbps)"]
[null,"Continuous recordable time (Motion images)",null,null,null,"AVCHD with picture quality set to [FSH]: Approx. 160 min with H-FS014042 / Approx. 170 min with H-H014"]
[null,"Actual recordable time (Motion images)",null,null,null,"AVCHD with picture quality set to [FSH]: Approx. 130 min with H-FS014042 / Approx. 150 min with H-H014"]
["FOCUS","Type",null,null,null,"Contrast AF system"]
[null,"Focus mode",null,null,null,"AFS/ AFC/ MF "]
[null,"AF mode",null,null,null,"Face detection / AF Tracking / 23-area-focusing / 1-area-focusing/Pinpoint\n"]
[null,"AF detective range",null,null,null,"EV 0 - 18 (ISO100 equivalent)"]
[null,"AF assist lamp",null,null,null,"YES"]
[null,"AF lock",null,null,null,"Set the Fn button in custom menu to AF lock"]
[null,"Others",null,null,null,"Quick AF, Continuous AF (during motion image recording), AF+MF, Touch shutter, Touch MF Assist,"]
["EXPOSURE CONTROL","Light metering system",null,null,null,"144-zone multi-pattern sensing system"]
[null,"Light metering mode",null,null,null,"Intelligent Multiple / Center Weighted / Spot "]
[null,"Metering range",null,null,null,"EV 0 - 18 (F2.0 lens, ISO100 equivalent)"]
[null,"Exposure mode",null,null,null,"Program AE, Aperture Priority AE, Shutter Priority AE, Manual, "]
[null,"ISO sensitivity(Standard Output Sensitivity)",null,null,null,"Auto / Intelligent ISO / 160 / 200 / 400 / 800 / 1600 / 3200 / 6400"]
[null,"Exposure compensation",null,null,null,"1/3EV Step ±3EV"]
[null,"AE lock",null,null,null,"Set the Fn button in custom menu to AE lock"]
[null,"AE bracket",null,null,null,"3,5 frame, in 1/3 or 2/3 EV Step, ±4/3 EV"]
["WHITE BALANCE","White balance",null,null,null,"Auto / Daylight / Cloudy / Shade / Halogen / Flash / White Set 1, 2 / Color temperature setting / Portrait / Beauty skin / Sport / Flower / Collection / Baby / Pet / defocus control"]
[null,"White balance adjustment",null,null,null,"Blue/amber bias, Magenta/green bias"]
[null,"Color temperature setting",null,null,null,"2500-10000K in 100K"]
[null,"White balance bracket",null,null,null,"3 exposures in blue/ amber axis or in magenta/ green axis"]
["SHUTTER","Type",null,null,null,"Focal-plane shutter"]
[null,"Shutter speed",null,null,null,"Still Images: 1/4000 ~ 60 \nMotion image: 1/16000 ~ 1/30 (NTSC),  1/16000 ~ 1/25 (PAL)"]
[null,"Self timer",null,null,null,"10sec, 3 images/  2sec / 10sec "]
["SCENE MODE","Still Image SCN mode",null,null,null,"Portrait / Soft Skin / Scenery / Architecture / Sports / Peripheral Defocus / Flower / Food / Objects / /Night Portrait / Night Scenery / Illiminatioms / Baby 1, 2 / Pet / Party / Sunset"]
[null,"Movie SCN mode",null,null,null,"Portrait / Soft Skin / Scenery / Architecture / Sports / Flower / Food / Objects / Low-light / Party / Sunset\n(Activated by selecting Still Image SCN mode then pressing Movie Button. Still Image SCN modes without corresponding Movie SCN mode is recorded in mode suitable for the recording situation.)"]
["BURST SHOOTING","Burst speed",null,null,null,"H: 3.8 frames/sec, M: 2.8 frames/sec (with Live View), L: 2 frames/sec (with Live View)"]
[null,"Number of recordable images",null,null,null,"7 images (when there are RAW files with the particular speed) "]
[{"$nulls":5},"Unlimited consecutive shooting (when there are no RAW files)"]
[{"$nulls":5},"(depending on memory card size, battery power, picture size, and compression)"]
["BUILT-IN-FLASH","Type",null,null,null,"TTL Built-in-Flash, GN6.3 equivalent (ISO 160 ・m), Built-in Pop-up"]
[null,"Flash mode",null,null,null,"Auto, Auto/Red-eye Reduction, Forced On, Forced On/Red-eye Reduction,"]
[{"$nulls":5},"Slow Sync., Slow Sync./Red-eye Reduction, Forced Off"]
[null,"Synchronization speed",null,null,null,"Less than 1/160 second"]
[null,"Flash synchronization",null,null,null,"1st. Curtain Sync"]
["LCD MONITOR","Type",null,null,null,"TFT LCD with Touch panel"]
[null,"Monitor size",null,null,null,"3.0inch / 3:2 Aspect / Wide-viewing angle "]
[null,"Pixels",null,null,null,"460K dots"]
[null,"Field of view",null,null,null,"Approx. 100%"]
[null,"Monitor adjustment",null,null,null,"Brightness (7 levels), Cnotrast and Saturation (7 levels), Red tint (7 levels), Blue tint (7 levels)"]
["LIVE VIEW","Digital zoom",null,null,null,"2x, 4x"]
[null,"Extra Tele Conversion ",null,null,null,"Still image: Max.2x (Not effective with L size recording. Magnification ratio depends on the recording pixels and aspect ratio.)\nMotion image: 3.1x (SH/H in AVCHD and HD/WVGA in Motion JPEG), 4.2x (VGA/QVGA in Motion JPEG)"]
[null,"Other functions",null,null,null,"Guide Lines (3 patterns)"]
[{"$nulls":5},"Real-time Histogram"]
["CREATIVE CONTROL","Creative control",null,null,null,"(Still image & Motion image) Expressive / Retro / High key / Sepia / High Dyamic / Miniature"]
["PLAYBACK","Playback mode",null,null,null,"Normal playback, 30-thumbnail display, 12-thumbnail display, Calendar display, Zoomed playback (16x Max.), Slideshow (duration & effect is selectable), Playback Mode (Normal/Picture/AVCHD/Motion JPEG/3D Play/Category/Favorite), Title Edit, Text Stamp, Video Divide, Resize, Cropping, Aspect Conversion, Rotate, Rotate Display, Favorite, Print set, Protect, Face Recognition Edit"]
["IMAGE PROTECTION / ERASE","Protection",null,null,null,"Single / Multi, Single in Burst Group / Multi in Burst Group, Cancel"]
[null,"Erase",null,null,null,"Single / Multi / All / Except Favorite"]
["PRINT","Direct print",null,null,null,"PictBridge compatible（Print size, Layout, Date setting are selectable ）"]
["INTERFACE","USB",null,null,null,"USB 2.0 High Speed"]
[null,"HDMI",null,null,null,"miniHDMI TypeC\nVideo: Auto / 1080i / 720p / 480p (576p in PAL system)\nAudio: Linear PCM"]
[null,"Audio video output",null,null,null,"Monaural Type, NTSC/PAL, NTSC only for North America\n*Check the website of the Panasonic sales company in your country or region for details on the products that are available in your market."]
[null,"Microphone",null,null,null,"Monaural, Wind-cut: Off / Low / Standard / High\nMicrophone level adjustable: Lv1 / Lv2 / Lv3 / Lv4"]
[null,"Speaker",null,null,null,"Monaural"]
["LANGUAGE","OSD language",null,null,null,"English, German, French, Italian, Spanish, Polish, Czech, Hungarian, Russian, Chinese (Traditional), Chinese (Simplified), \nDutch, Thai, Korean, Turkish, Portuguese, Arabic, Persian, Japanese, Swedish, Danish, Finnish, Greek, Vietnamese\n*Check the website of the Panasonic sales company in your country or region for details on the OSD languages on the products that are available in your market."]
["POWER","Battery",null,null,null,"Li-ion Battery Pack (7.2V, 940mAh)  (Included)"]
[{"$nulls":5},"Battery Charger"]
[null,"Battery life (CIPA standard)",null,null,null,"Approx. 320 images with H-FS014042\nApprox. 340 images with H-H014   "]
["DIMENSIONS / WEIGHT","Dimensions (W x H x D)",null,null,null,"107.7 x 67.1 x 32.5 mm / 4.24 x 2.64 x 1.28 inch　(excluding protrusions)"]
[null,"Weight",null,null,null,"Approx. 264g / 9.31 oz    （SD card, Battery, Body)\nApprox. 222g / 7.83 oz    （Body only)\nApprox. 319g / 11.25 oz  （SD card, Battery, H-H014 lens included） \nApprox. 429g / 15.13 oz   (SD card, Battery, H-FS014042 lens included)"]
["OPERATING ENVIRONMENT","Operating temperature",null,null,null,"0℃ to 40℃ (32°F to 104°F)"]
[null,"Operating humidity",null,null,null,"10% to 80％"]
["STANDARD ACCESSORIES","Software",null,null,null,"PHOTOfunSTUDIO 6.2 HD Edition"]
[{"$nulls":5},"SILKYPIX® Developer Studio 3.1 SE\nSuper LoiloScope (trial version)"]
[{"$nulls":5},"USB Driver"]
[null,"Standard accessories",null,null,null,"Battery Charger, Body Cap(DMC-GF3K and DMC-GF3 only), "]
[{"$nulls":5},"AV Cable, USB Connection Cable, Shoulder Strap, Stylus pen, CD-ROM\n*   Body cap not included for DMC-GF3C kit and DMC-GF3W kit\n** Lens rear cap of H-H014 lens not included for DMC-GF3C kit and DMC-GF3W Kit "]
["*1 Use a card with SD Speed Class with \"Class6\" or higher"]
["*2 Use a card with SD Speed Class with \"Class4\" or higher"]