{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["history","L1 (Eur)","Dlens (Eur)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"history","index":0,"n_rows":7,"n_cols":5,"rows_kept":7,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"2006-06-15","addition","L1","Digital zoom "]
[null,null,"addition","L1","Extra optical zoom"]
[null,null,"change","L1","Dimensions (D)"]
[null,null,"change","Dlens","weight"]

{"sheet":"L1 (Eur)","index":1,"n_rows":96,"n_cols":5,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Specifications of Digital Still Camera",null,null,"Ver. 2006.6.15.20:00"]
[null,null,null,"DMC-L1"]
[null,"TYPE","Type","Interchangeable Lens Digital SLR Camera"]
[null,null,"Recording Media","SD Memory Card, SDHC Memory Card, Multimedia Card"]
[null,null,"Image Sensor Size","17.3 x 13.0 mm"]
[null,null,"Mount","Four Thirds mount"]
[null,"IMAGE SENSOR","Type","Live Mos Sensor"]
[null,null,"Total Pixels","7.9 Mega-pixel"]
[null,null,"Camera Effective pixels","7.5 Mega-pixel"]
[null,null,"Aspect Ratio","3:4 (Vertical : Horizontal)"]
[null,null,"Color Filter","Primary color filter"]
[null,null,"Dust Reduction System","Supersonic Web Filter"]
[null,"RECORDING SYSTEM","Recording File Format","JPEG(Design rule for Camera File system, based on Exif 2.21 standard), "]
[null,null,null,"DPOF corresponding, RAW"]
[null,null,"Aspect Ratio","4:3, 3:2, 16:9 (3:2,16:9 with Live view only)"]
[null,null,"File Size"," 4:3 Aspect Ratio: 3136 x 2352 pixels, 2560 x 1920 pixels, 2048 x 1536 pixels"]
[null,null,null," 3:2 Aspect Ratio: 3136 x 2080 pixels,  2560 x 1712 pixels, 2048 x 1360 pixels"]
[null,null,null," 16:9 Aspect Ratio: 3136 x 1760 pixels, 1920 x 1080 pixels"]
[null,null,"Color Space","sRGB, Adobe RGB"]
[null,"VIEWFINDER","Type","Eye level Porro Mirror type Optical View Finder"]
[null,null,"Field of View","Apporox. 95%"]
[null,null,"Magnification","Apporox. 0.93x"]
[null,null,"Eye point","Approx.18mm (-1[m-1])"]
[null,null,"Diopter Adjustment","-3.0 ~ +1 [m-1]"]
[null,null,"Focusing Screen","Fixed type"]
[null,null,"Mirror","Quick Return Mirror"]
[null,null,"Depth-of-Field Preview","Enabled with Aperture Preview button (with Live view only)"]
[null,null,"Eyepiece Shutter","Detachable"]
[null,"AUTO FOCUS","Type","TTL Phase Difference Detection System"]
[null,null,"Focusing Mode","AFS/AFC/MF"]
[null,null,"Focusing Area","3 points"]
[null,null,"Focusing Area Selection","Auto / 1fixed point, left / 1fixed point, center/ 1fixed point, right"]
[null,null,"AF Detective Range","EV0-19 (ISO100)"]
[null,null,"AF Assist Lamp","YES"]
[null,null,"AF Lock","AFL/AEL button　or Shutter button halfway pressed in AFS mode"]
[null,"EXPOSURE CONTROL","Light Metering System","TTL Full Aperture Light Metering by "]
[null,null,null,"49 Zones Multi-pattern Sensing system(Optical view finder )"]
[null,null,null,"256 zone Multi-pattern Sensing system (Live view mode)"]
[null,null,"Light Metering Mode","Intelligent Multiple/ Center Weighted/ Spot "]
[null,null,"Metering Range","0 - 20EV with Optical view finder), 0 - 16EV with Live view mode (with F2.0 lens, ISO 100) "]
[null,null,"Exposure Mode"," Program AE / Aperture Priority AE/ Shutter Priority AE / Manual"]
[null,null,"ISO sensitivity","Auto/100/200/400/800/1600"]
[null,null,"Exposure Compensation","1/3EVStep ±2EV"]
[null,null,"AE Lock","AFL/AEL Button　or Shutter button halfway pressed"]
[null,null,"AE Bracket","3frame、5frame　1/3~1EV Step  ±2EV"]
[null,"WHITE BALANCE","White Balance","Auto  / Daylight / Cloudy / Shade / Halogen / Flash / White Set 1,2 / Color temperature setting"]
[null,null,"White Balance Adjustment","blue/amber bias, magenta/green bias"]
[null,null,"Color temperature setting","2500K to 10000K in 31steps"]
[null,"SHUTTER SYSTEM","Type","Focal-plane shutter"]
[null,null,"Shutter Speed","1/4000 ~ 60 and Bulb (up to approx. 8minutes)"]
[null,null,"Self Timer","10 sec / 2sec"]
[null,null,"Remote Control","Remote control with bulb function by DMW-RSL1 (Optional)"]
[null,"BURST SHOOTING","Burst Speed","3 frames/sec or 2 frames/sec"]
[null,null,"Number of Recordable","6 pictures (when there are RAW file), "]
[null,null,null,"Unlimited consecutive shooting (when there are no RAW file)"]
[null,null,null,"(depending on memory card size, battery power, picture size, and compression)"]
[null,"BUILT-IN-FLASH","Type","TTL Built-in-Flash, GN10 (ISO100,m), Built-in Pop-up, Bounce flash"]
[null,null,"Built-in Flash","Auto, Auto/Red-eye Reduction, Forced On/Red-eye Reduction,"]
[null,null,null,"Slow Sync., Slow Sync./Red-eye Reduction, Forced On/Off"]
[null,null,"X-Sync speed","Less than 1/160 second"]
[null,null,"Flash output adjustment","1/3EVStep ±2EV"]
[null,null,"Flash synchronization","1st. Curtain Sync. and  2nd Curtain Sync.　（Selectable）"]
[null,null,"Hot Shoe","TTL Auto with FL360/FL500 (Optional)"]
[null,"LCD MONITOR","Type","Low temperature Polycrystalline TFT LCD"]
[null,null,"Monitor Size","2.5inch"]
[null,null,"Pixels","207K pixels"]
[null,null,"Filed of view","Approx. 100% in LIVE VIEW MODE"]
[null,null,"OSD language","English,German,French,Italian,Spanish,Polish,Czech,Hangarian,Japanese"]
[null,"LIVE VIEW","Type","YES ( LCD monitor can be used as view finder, with Live MOS sensor set to monitor mode."]
[null,null,"Digital zoom","2x, 4x (with Live view only)"]
[null,null,"Extra Optical zoom ","Max.1.5x \n(With Live view only. Not effective with full pixel recording.\nMagnification ratio depends on the recording pixels.)"]
[null,"FILM MODE","Color","Standard / Dynamic / Nature / Smooth Color"]
[null,null,"Black and White","Standard / Dynamic / Smooth Color"]
[null,"PLAYBACK","Playback Mode","Single / 9, 25-thumbnail display, Calendar display, "]
[null,null,null,"Zoomed playback (16x max.), /image rotation  (except for RAW)"]
[null,null,null,"Slide show (duration is adjustable, also manual controllable),"]
[null,null,null,"Playback of favorite pictures/ Resizing (selectable number of pixels)"]
[null,null,null,"Trimming / Protection / Aspect conversion /  DPOF print setting"]
[null,"PROTECTION / ERASE","Protection","Single / Multi or Cancel"]
[null,null,"Erase","Single / Multi / All"]
[null,"DIRECT PRINT","Print","PictBridge（Print size, Layout, Date setting is selectable ）"]
[null,"INTERFACE","Digital","USB 2.0 (High speed)"]
[null,null,"Analog Video","NTSC/PAL Composite (Switched by menu)"]
[null,"POWER","Battery","Li-ion Battery Pack (7.2V, 1500mAh)  (Included)"]
[null,null,null,"Battery Charger/AC Adaptor (Input: 110-240V AC) (Included)"]
[null,null,"Battery Life","Approx. 450 images　（CIPA Standard with LEICA D VARIO-ELMARIT 14-50mm/F2,8-F3.5 ASPH.）"]
[null,"DIMENSIONS / WIGHT","Dimensions (W x H x D)","145.8 x 86.9 x 80mm"]
[null,null,"Weight","Approx. 530g（Body only）"]
[null,"OPERATING CONDITION","Operating temperature","0℃ to 40℃"]
[null,null,"Operating humidity","10% to 80％"]
[null,"STANDARD ACCESSORY","Software","LUMIX Simple Viewer, PhotofunStudio -viewer-"]
[null,null,null,"SILKYPIX DEVELOPER STUDIO"]
[null,null,null,"Quick Time"]
[null,null,null,"USB Driver"]
[null,null,"Standard Accessory","Battery Charger/AC adaptor, Battery Pack, Eyepiece Cap, Body Cap,"]
[null,null,null,"Video Cable, USB Connection Cable, AC Cable, DC Cable, Strap, CD-ROM"]

{"sheet":"Dlens (Eur)","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Specifications of Leica D lens",null,"Ver. 2006.6.15.20:00"]
[null,null,"LEICA D VARIO-ELMARIT 14-50mm/F2,8-F3.5 ASPH."]
[null,"Lens Construction","16 elements in 12groups (2 Aspherical lenses)"]
[null,"Mount","Four Thirds mount"]
[null,"Optical Image Stabilizer ","YES"]
[null,null,"On/Off (selectable Mode1 /2 with only DMC-L1)"]
[null,"Focal Length","f=14mm to 50mm (35mm film camera equivalent 28mm to 100mm)"]
[null,"Aperture Type","7 diaphragm blades / iris diaphragm"]
[null,"Aperture Range","F2.8(wide) - F3.5(Tele)"]
[null,"Minimum Aperture","F22"]
[null,"Closest Focusing Distance","0.29m at all focal lengths"]
[null,"Maximum magnification ","Apporox. 0.32x (35mm Equiv)"]
[null,"Diagonal Angle of View","75°（Ｗ）～24°（Ｔ）"]
[null,"Filter Size","72mm"]
[null,"Max.Diameter","φ78.1 "]
[null,"Overall Length","102.8mm"]
[null,"Weight","490g"]
[null,"Standard Accessory","Lens Cap, Lens Hood, Lens Rear Cap, Lens Storage Bag"]