{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Technical Data"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Technical Data","index":0,"n_rows":105,"n_cols":11,"rows_kept":105,"cut":false,"hidden":false,"merged":[[5,0,5,10],[22,0,22,10],[0,0,0,10],[1,0,1,10],[2,0,2,10],[4,0,4,10],[88,0,88,10],[103,0,103,10],[23,0,23,10],[34,0,34,10],[35,0,35,10],[42,0,42,10],[43,0,43,10],[53,0,53,10],[54,0,54,10],[65,0,65,10],[66,0,66,10],[87,0,87,10]],"flags":["formulas_cached_only"]}
["Volvo Car Corporation"]
["2010 Volvo C30"]
["Technical Data"]
[" ","Petrol 1.6","Petrol 2.0","Petrol 2.4i","Petrol T5","Diesel DRIVe","Diesel DRIVe Start/Stop","Diesel 2.0D","Diesel D5","Diesel D5","Ethanol/Petrol 2.0F"]
[" "]
["Engine"]
["Engines","B4164S3","B4204S3","B5244S4","B5254T7","D4164T","D4164T","D4204T","D5244T13","D5244T8","B4204S4"]
["Type","4 cyl. Petrol. Naturally aspirated","4 cyl. Naturally aspirated","5 cyl . Naturally aspirated","In-line 5 cyl. Turbo","In-line 4 cyl. Turbo","In-line 4 cyl. Turbo","In-line 4 cyl. Turbo","In-line 5 cyl. Turbo","In-line 5 cyl. Turbo","4 cyl. Naturally aspirated"]
["Configuration","FWD","FWD","FWD","FWD","FWD","FWD","FWD","FWD","FWD","FWD"]
["Displacement","1596 cm³","1999 cm³","2435 cm³","2521 cm³","1560 cm³","1560 cm³","1997 cm³","2400 cm³","2400 cm³","1999 cm³"]
["Bore","79 mm","87,5 mm","83 mm","83 mm","75 mm","75 mm","85 mm","81 mm","81 mm","87,5 mm"]
["Stroke","81,4 mm","83,1 mm","90 mm","93,2 mm","88,3 mm","88,3 mm","88 mm","93,15 mm","93,15 mm","83,1 mm"]
["Compression ratio","11,0:1","10,8:1","10,3:1","9,0:1","18,3:1","18,3:1","18,5:1","17,3:1","17,3:1","10,8:1"]
["Valves, no/cylinder","4 ea.","4 ea.","4 ea.","4 ea.","4 ea.","4 ea.","4 ea.","4 ea.","4 ea.","4 ea."]
["DOHC / SOHC","DOHC","DOHC","DOHC","DOHC","DOHC","DOHC","DOHC","DOHC","DOHC","DOHC"]
["Engine management system","Integrated fuel (SFI) / ignition control system","Integrated fuel (SFI) / ignition control system","Integrated fuel (SFI) / ignition control system","Integrated fuel (SFI) / ignition control system","Common rail electronic fuelling","Common rail electronic fuelling","Common rail electronic fuelling","Common rail electronic fuelling","Common rail electronic fuelling","Integrated fuel (SFI) / ignition control system"]
["Ignition sequence","1-3-4-2","1-3-4-2","1-2-4-5-3","1-2-4-5-3","1-3-4-2","1-3-4-2","1-3-4-2","1-2-4-5-3","1-2-4-5-3","1-3-4-2"]
["Engine idling speed","725 rpm","700 rpm","720 rpm","770 rpm","790 rpm","790 rpm","800 rpm","720 rpm","720 rpm","700 rpm"]
["Fuel, rec. Octane","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","Diesel. Cetane Number min 48","Diesel. Cetane Number min 48","Diesel. Cetane Number min 48","Diesel. Cetane Number min 48","Diesel. Cetane Number min 48","E85 is recommended (Mixture 15 % Petrol and 85 % Ethanol)"]
["Max engine speed","6450 rpm","6450 rpm","6500 rpm","6500 rpm","5000 rpm","5000 rpm","4800 rpm","5000 rpm","5000 rpm","6450 rpm"]
["Max output","74 kW (100 hp) / 6000 rpm","107 kW (145 hp) / 6000 rpm","125 kW (170 hp) / 6000 rpm","169 kW (230 hp) / 5000 rpm","80 kW (109 hp) / 4000 rpm","80 kW (109 hp) / 4000 rpm","100 kW (136 hp) / 4000 rpm","132 kW (180 hp) / 4000 rpm","132 kW (180 hp) / 4000 rpm","107 kW (145 hp) / 6000 rpm"]
["Max torque","150 / 67 Nm / rps","185 / 75 Nm / rps","230 / 73 Nm / rps","320 / 25-83 Nm / rps","240 / 29 Nm / rps","240 / 29 Nm / rps","320 / 33 Nm / rps","400 / 33 - 46 Nm / rps","350 / 29-54 Nm / rps","185 / 75 Nm / rps"]
[" "]
["Transmissions"]
["Transmissions","IB5","MTX75 Q1 / MPS6-2","M56H / AW55-51","M66W / AW55-51","MTX75 D1","MTX75 D1","MMT6  W3 / M56L2 / MPS6-4","M66D","AW55 -51","MTX75 Q1"]
["First Gear",3.583,"3,417 / 3,583","3,071 / 4,657","3,385 / 4,657",3.8,3.8,"3,583 / 3,385 / 3,583",3.385,4.657,3.417]
["Second Gear",2.038,"2,136 / 2,048","1,773 / 3,032","1,905 / 3,032",2.048,2.048,"1,952 / 1,905 / 1,952",1.905,3.032,2.136]
["Third Gear",1.414,"1,448 / 1,370","1,194 / 1,982","1,267 / 1,982",1.258,1.258,"1,241 / 1,194 / 1,194",1.194,1.982,1.448]
["Fourth Gear",1.108,"1,028 / 1,029","0,868 / 1,341","0,949 / 1,341",0.865,0.865,"0,868 / 0,868 / 0,842",0.838,1.341,1.028]
["Fifth Gear",0.878,"0,805 / 1,161","0,700 / 1,018","0,775 / 1,018",0.674,0.674,"0,943 / 0,652 / 0,943",0.652,1.018,0.805]
["Sixth Gear","-","- / 0,971","- / -","0,652 / -","-","-","0,789 / - / 0,789",0.54,"-","-"]
["Reverse Gear",3.615,"3,727 / 4,843","2,993 / 5,114","3,197 / 5,114",3.727,3.727,"5,099 / 3,298 / 4,843",3.231,5.114,3.727]
["Manual Gearbox/final drive",4.06,4.067,4.25,3.77,3.41,3.41,"3,813 (Gear 1-4) / 2,773 (Gear 5-6 + R) / 3,770",4,"-",4.067]
["Automatic Gearbox/final drive","-","4,533 (Gear 1-4) - 3,238 (Gear 5-6+R)",2.44,2.27,"-","-","4,067 (Gear 1-4) / 2,905 (Gear 5-6+R)","-",2.27,"-"]
[" "]
["Performance"]
["Performance","Manual","Manual / Automatic","Manual / Automatic","Manual / Automatic","Manual","Manual","Manual / Manual / Automatic","Manual","Automatic","Manual"]
["Gearbox","IB5","MTX75 Q1 / MPS6-2","M56H / AW55-51","M66W / AW55-51","MTX75 D1","MTX75 D1","MMT6  W3 / M56L2 / MPS6-4","M66D","AW55-51","MTX75 Q1"]
["Acceleration, 0-100 km/h","11,8 sec","9,4 sec / 9,7 sec","8,1 sec / 8,8 sec","6,7 sec / 7,1 sec","11,3 sec","11,3 sec","9,4 sec / 9,4 sec / 9,5 sec","7,7 sec","8,4 sec","9,4 sec"]
["Top speed","185 km/h","210 km/h /  205 km/h","220 km/h / 215 km/h","240 km/h / 235 km/h","190 km/h","190 km/h","205 km/h / 205 km/h / 205 km/h","220 km/h","220 km/h","210 km/h"]
["Fuel consumption (EC 199/100, Combined)","7,0 l/100km","7,6 l/100km / 8,1 l/100km","8,4 l/100km / 9,0 l/100km","8,7 l/100km / 9,0 l/100km","4,5 l/100km","3,8 l/100km","5,7 l/100km / 5,5 l/100km / 5,9 l/100km","6,2 l/100km","6,9 l/100km","7,8 l/100km (petrol) / 10,9 l/100km E85. (Value not certified)"]
["CO²","167 g/km","177 g/km / 194 g/km","200 g/km / 214 g/km","203 g/km / 211 g/km","119 g/km","99 g/km","151 g/km / 146 g/km / 156 g/km","164 g/km","182 g/km","185 g/km (pet) / 178 g/km E85. (Value not certified)"]
[" "]
["Measurements and Volumes"]
["Length","4266 mm","4266 mm","4266 mm","4266 mm","4266 mm","4266 mm","4266 mm","4266 mm","4266 mm","4266 mm"]
["Width (Incl mirrors, folded)","1871 mm","1871 mm","1871 mm","1871 mm","1871 mm","1871 mm","1871 mm","1871 mm","1871 mm","1871 mm"]
["Width (Incl mirrors, outer edge)","2039 mm","2039 mm","2039 mm","2039 mm","2039 mm","2039 mm","2039 mm","2039 mm","2039 mm","2039 mm"]
["Height (incl shark fen)","1447 mm","1447 mm","1447 mm","1447 mm","1447 mm","1447 mm","1447 mm","1447 mm","1447 mm","1447 mm"]
["Wheelbase","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm"]
["Track, front (15\") &(16\"/17\")","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm","1548 mm / 1535 mm"]
["Track, rear (15\") & (16\"/17\")","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm","1544 mm / 1531 mm"]
["Ground clearance","135 mm","135 mm","135 mm","135 mm","135 mm","135 mm","135 mm","135 mm","135 mm","135 mm"]
["Cargo floor height to ground","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm"]
[" "]
["Weight/Miscellaneous"]
["Serving Weight (Depending on type of engine, gearbox etc.)","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg","1275 kg / 1471 kg"]
["Total Weight (Depending on type of engine, gearbox etc.)","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg","1700 kg / 1900 kg"]
["Max trailer weight, Unbraked (Max)","600 kg","650 kg","700 kg","700 kg","650 kg","0 kg","700 kg","700 kg","700 kg","700 kg"]
["Max trailer weight, Braked (Max)","1200 kg","1350 kg","1500 kg","1500 kg","1300 kg","0 kg","1500 kg","1500 kg","1500 kg","1350 kg"]
["Fuel tank, Petrol","55 l","55 l","62 l","62 l","-","-","-","-","-","-"]
["Fuel tank, Diesel","-","-","-","-","52 l","52 l","52 l","60 l","60 l","-"]
["Fuel tank, E85","-","-","-","-","-","-","-","-","-","55 l"]
["Aerodynamics, (Cd)",0.31,0.31,0.31,0.31,0.28,0.28,0.31,0.31,0.31,0.31]
["Aerodynamics, (Frontal area)","2,18 m²","2,18 m²","2,18 m²","2,18 m²","2,18 m²","2,18 m²","2,18 m²","2,18 m²","2,18 m²","2,18 m²"]
["Max roof load","75 kg","75 kg","75 kg","75 kg","75 kg","75 kg","75 kg","75 kg","75 kg","75 kg"]
[" "]
["Interior Measurements"]
["Headroom with sunroof (front/rear)","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm","965 mm / 959 mm"]
["Headroom without sunroof (front/rear)","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm","988 mm / 959 mm"]
["Passenger compartment width at shoulder height (front/rear)","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm","1390 mm / 1303 mm"]
["Leg room (front/rear)","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm","1057 mm / 869 mm"]
["Luggage volume, Variants with Spare wheel / including under floor volume. (According to ISO V211)","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l","233 l / 9 l"]
["Luggage volume, Variants with Repair kit / including under floor volume. (According to ISO V211)","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l","251 l / 27 l"]
["Luggage volume, Variants with Spare wheel / including under floor volume. (According to ISO V212)","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l","521 l / 9 l"]
["Luggage volume, Variants with Repair kit / including under floor volume. (According to ISO V212)","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l","539 l / 27 l"]
["Luggage volume, Variants with Spare wheel / including under floor volume. (According to ISO V214)","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l","876 l / 9 l"]
["Luggage volume, Variants with Repair kit / including under floor volume.(According to ISO V214)","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l","894 l / 27 l"]
["Luggage floor, height to ground.","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm","654 mm"]
["Lift over height","807 mm","807 mm","807 mm","807 mm","807 mm","807 mm","807 mm","807 mm","807 mm","807 mm"]
["Rear opening height","470 mm","470 mm","470 mm","470 mm","470 mm","470 mm","470 mm","470 mm","470 mm","470 mm"]
["Height of luggage compartment","642 mm","642 mm","642 mm","642 mm","642 mm","642 mm","642 mm","642 mm","642 mm","642 mm"]
["Width of luggage compartment between wheelhouses","954 mm","954 mm","954 mm","954 mm","954 mm","954 mm","954 mm","954 mm","954 mm","954 mm"]
["Rear opening width at floor, min.","713 mm","713 mm","713 mm","713 mm","713 mm","713 mm","713 mm","713 mm","713 mm","713 mm"]
["Rear opening width above belt, min.","778 mm","778 mm","778 mm","778 mm","778 mm","778 mm","778 mm","778 mm","778 mm","778 mm"]
["Rear opening maximum width","897 mm","897 mm","897 mm","897 mm","897 mm","897 mm","897 mm","897 mm","897 mm","897 mm"]
["Load length from the second seatback to the rearmost point","711 mm","711 mm","711 mm","711 mm","711 mm","711 mm","711 mm","711 mm","711 mm","711 mm"]
["Load length from the first seatback to the rearmost point","1534 mm","1534 mm","1534 mm","1534 mm","1534 mm","1534 mm","1534 mm","1534 mm","1534 mm","1534 mm"]
[" "]
["Chassis"]
["Suspension front","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar"]
["Suspension rear","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar"]
["Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering","Power Assisted Rack and Pinion Steering"]
["Turning circle 16\" (Curb to curb)","10,6 m","10,6 m","10,6 m","10,6 m","10,6 m","10,6 m","10,6 m","10,6 m","10,6 m","10,6 m"]
["Turning circle 18\" (Curb to curb)","11,6 m","11,6 m","11,6 m","11,6 m","11,6 m","11,6 m","11,6 m","11,6 m","11,6 m","11,6 m"]
["Turning circle 16\" (Wall to wall)","11,1 m","11,1 m","11,1 m","11,1 m","11,1 m","11,1 m","11,1 m","11,1 m","11,1 m","11,1 m"]
["Turning circle 18\" (Wall to wall)","12,1 m","12,1 m","12,1 m","12,1 m","12,1 m","12,1 m","12,1 m","12,1 m","12,1 m","12,1 m"]
["Turns of steering wheel end to end, 16\"",2.9,2.9,2.9,2.9,2.9,2.9,2.9,2.9,2.9,2.9]
["Turns of steering wheel end to end, 18\"",2.6,2.6,2.6,2.6,2.6,2.6,2.6,2.6,2.6,2.6]
["Braking system","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)"]
["Brake disc diameter (front ventilated)","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm","278 mm / 300 mm"]
["Brake disc diameter (rear solid)","280 mm","280 mm","280 mm","280 mm","280 mm","280 mm","280 mm","280 mm","280 mm","280 mm"]
["Brake disc thickness (front/rear)","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm","25 mm / 11 mm"]
["Braking distance 100-0 km/h","38  m","38 m","38 m","38 m","38 m","38 m","38 m","38 m","38 m","38 m"]
[" "]
["All figures are preliminary. Volvo reserves the right to make changes in the specifications without any notice."]