{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Technical Data"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Technical Data","index":0,"n_rows":87,"n_cols":7,"rows_kept":87,"cut":false,"hidden":false,"merged":[[72,0,72,6],[85,0,85,6],[52,0,52,6],[62,0,62,6],[63,0,63,6],[71,0,71,6],[34,0,34,6],[40,0,40,6],[41,0,41,6],[51,0,51,6],[5,0,5,6],[21,0,21,6],[22,0,22,6],[33,0,33,6],[0,0,0,6],[1,0,1,6],[2,0,2,6],[4,0,4,6]],"flags":["formulas_cached_only"]}
["Volvo Car Corporation"]
["2010 Volvo C70"]
["Technical Data"]
[" ","Petrol 2.4","Petrol 2.4i","Petrol T5","Diesel 2.0 D","Diesel D5 (Manual)","Diesel D5"]
[" "]
["Engine"]
["Engines","B5244S5","B5244S4","B5254T7","D4204T","D5244T13","D5244T8"]
["Type","5 cyl. Naturally aspirated","5 cyl. Naturally aspirated","In-line 5 cyl. Turbo","In-line 4 cyl. Turbo","In-line 5 cyl. Turbo","In-line 5 cyl. Turbo"]
["Configuration","FWD","FWD","FWD","FWD","FWD","FWD"]
["Displacement","2435 cm³","2435 cm³","2521 cm³","1997 cm³","2400 cm³","2400 cm³"]
["Bore","83 mm","83 mm","83 mm","85 mm","81 mm","81 mm"]
["Stroke","90 mm","90 mm","93,2 mm","88 mm","93,15 mm","93,15 mm"]
["Compression ratio","10,3:1","10,3:1","9,0:1","18,5:1","17,3:1","17,3:1"]
["Valves, no/cylinder","4 ea.","4 ea.","4 ea.","4 ea.","4 ea.","4 ea."]
["DOHC / SOHC","DOHC","DOHC","DOHC","DOHC","DOHC","DOHC"]
["Engine management system","Integrated fuel (SFI) / ignition control system","Integrated fuel (SFI) / ignition control system","Integrated fuel (SFI) / ignition control system","Common rail electronic fuelling","Common rail electronic fuelling","Common rail electronic fuelling"]
["Ignition sequence","1 - 2 - 4 - 5 - 3","1 - 2 - 4 - 5 - 3","1 - 2 - 4 - 5 - 3","1 - 3 - 4 - 2","1 - 2 - 4 - 5 - 3","1 - 2 - 4 - 5 - 3"]
["Engine idling speed","720 rpm","720 rpm","770 rpm","800 rpm","720 rpm","720 rpm"]
["Fuel, rec. Octane","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","For best performance and lowest fuel consumption 98 RON is recommended. For normal driving 95 RON can be used. 91 RON should only be used in exceptional cases.","Diesel. Cetane Number min 48","Diesel. Cetane Number min 48","Diesel. Cetane Number min 48"]
["Max output","103 kW (140 hp) / 5000 rpm","125 kW (170 hp) / 6000 rpm","169 kW (230 hp) / 5000 rpm","100 kW (136 hp) / 4000 rpm","132 kW (180 hp) / 4000 rpm","132 kW (180 hp) / 4000 rpm"]
["Max torque","220 / 67 Nm / rps","230 / 73 Nm / rps","320 / 25-83 Nm / rps","320 / 33 Nm / rps","400 / 33-46 Nm / rps","350 / 29-54 Nm / rps"]
[" "]
["Transmissions"]
["Transmissions","M56L / AW55-51","M56H / AW55-51","M66W / AW55-51","MMT6 W3 / MPS6-4","M66D","AW55-51"]
["First Gear","3,385 / 4,657","3,071 / 4,657","3,385 / 4,657","3,583 / 3,583",3.385,4.657]
["Second Gear","1,905 / 3,032","1,773 / 3,032","1,905 / 3,032","1,952 / 1,952",1.905,3.032]
["Third Gear","1,194 / 1,982","1,194 / 1,982","1,267 / 1,982","1,241 / 1,194",1.194,1.982]
["Fourth Gear","0,868 / 1,341","0,868 / 1,341","0,949 / 1,341","0,868 / 0,842",0.838,1.341]
["Fifth Gear","0,700 / 1,018","0,700 / 1,018","0,775 / 1,018","0,943 / 0,943",0.652,1.018]
["Sixth Gear","- / -","- / -","0,652 / -","0,786 / 0,789",0.54,"-"]
["Reverse Gear","3,298 / 5,114","2,993 / 5,114","3,197 / 5,114","5,099 / 4,843",3.231,5.114]
["Manual Gearbox/final drive",4,4.25,3.77,"3,813 (Gear 1-4) / 2,773 (Gear 5-6 + R)",4,"-"]
["Automatic Gearbox/final drive",2.44,2.44,2.27,"4,067 (Gear 1-4) / 2,905 (Gear 5-6 + R)","-",2.27]
[" "]
["Performance"]
["Gearbox","Manual / Automatic","Manual / Automatic","Manual / Automatic","Manual / Automatic","Automatic","Automatic"]
["Acceleration, 0-100 km/h","11,0 s / 11,8 s","9,1 s / 10,0 s","7,6 s / 8,0 s","11,0 s / 11,1 s","9,0 s","9,5 s"]
["Top speed","205  km/h / 200 km/h","220 km/h / 215 km/h","240 km/h / 235 km/h","205 km/h / 205 km/h","225 km/h","220 km/h"]
["Fuel consumption (EC 199/100, Combined)","8,9 l/100km / 9,6 l/100km","9,0 l/100km / 9,6 l/100km","8,9 l/100km / 9,4 l/100km","6,0 l/100km / 6,3 l/100km","6,6 l/100km","7,3 l/100km"]
["CO²","212 g/km / 229 g/km","215 g/km / 229 g/km","209 g/km / 219 g/km","158 g/km / 167 g/km","174 g/km","193 g/km"]
[" "]
["Measurements and Volumes"]
["Length","4615 mm","4615 mm","4615 mm","4615 mm","4615 mm","4615 mm"]
["Width (incl mirrors, folded)","1836 mm","1836 mm","1836 mm","1836 mm","1836 mm","1836 mm"]
["Width (incl. mirrors outer edge)","2025 mm","2025 mm","2025 mm","2025 mm","2025 mm","2025 mm"]
["Height","1400 mm","1400 mm","1400 mm","1400 mm","1400 mm","1400 mm"]
["Height during roof operation","approx. 2000 mm","approx. 2000 mm","approx. 2000 mm","approx. 2000 mm","approx. 2000 mm","approx. 2000 mm"]
["Wheelbase","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm","2640 mm"]
["Track, front","1550 mm","1550 mm","1550 mm","1550 mm","1550 mm","1550 mm"]
["Track, rear","1560 mm","1560 mm","1560 mm","1560 mm","1560 mm","1560 mm"]
["Ground clearance","140 mm","140 mm","140 mm","140 mm","140 mm","140 mm"]
[" "]
["Weight/Miscellaneous"]
["Serving Weight (Depending on type of engine, gearbox etc.)","1681 kg / 1760 kg","1681 kg / 1760 kg","1681 kg / 1760 kg","1681 kg / 1760 kg","1681 kg / 1760 kg","1681 kg / 1760 kg"]
["Total Weight (Depending on type of engine, gearbox etc.)","2070 kg / 2150 kg","2070 kg / 2150 kg","2070 kg / 2150 kg","2070 kg / 2150 kg","2070 kg / 2150 kg","2070 kg / 2150 kg"]
["Max trailer weight, Unbraked (Max)","750 kg","750 kg","750 kg","750 kg","750 kg","750 kg"]
["Max trailer weight, Braked (Max)","1500 kg","1500 kg","1500 kg","1500 kg","1500 kg","1500 kg"]
["Fuel tank, Petrol","62 l","62 l","62 l","-","-","-"]
["Fuel tank, Diesel","-","-","-","52 l","60 l","60 l"]
["Aerodynamics, (Cd)",0.31,0.31,0.31,0.31,0.31,0.31]
["Aerodynamics, (Frontal area)","2,13 - 2,15 m²","2,13 - 2,15 m²","2,13 - 2,15 m²","2,13 - 2,15 m²","2,13 / 2,15 m²","2,13 - 2,15 m²"]
["Headroom with roof closed (front/rear)","970 mm / 924 mm","970 mm / 924 mm","970 mm / 924 mm","970 mm / 924 mm","970 mm / 924 mm","970 mm / 924 mm"]
[" "]
["Interior Measurements"]
["Passenger compartment width at shoulder height (front/rear)","1361 mm / 1194 mm","1361 mm / 1194 mm","1361 mm / 1194 mm","1361 mm / 1194 mm","1361 mm / 1194 mm","1361 mm / 1194 mm"]
["Leg room (front/rear)","1074 mm / 862 mm","1074 mm / 862 mm","1074 mm / 862 mm","1074 mm / 862 mm","1074 mm / 862 mm","1074 mm / 862 mm"]
["Luggage volume, roof closed/open","404 l / 200 l","404 l / 200 l","404 l / 200 l","404 l / 200 l","404 l / 200 l","404 l / 200 l"]
["Cargo length at floor from the back of the rear torsional wall","850 mm","850 mm","850 mm","850 mm","850 mm","850 mm"]
["Loading height between cargo floor and trunk divider roof closed/open","525 mm / 265 mm","525 mm / 265 mm","525 mm / 265 mm","525 mm / 265 mm","525 mm / 265 mm","525 mm / 265 mm"]
["Lift over height to enter luggage compartment","680 mm","680 mm","680 mm","680 mm","680 mm","680 mm"]
["Width of luggage compartment between wheelhouses","960 mm","960 mm","960 mm","960 mm","960 mm","960 mm"]
[" "]
["Chassis"]
["Suspension front","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","MacPherson Strut, Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar"]
["Suspension rear","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar","Independent Suspension with Coil Springs, Hydraulic Shock Absorbers, Stabilizer Bar"]
["Steering ratio (angle/angle)","15,3:1","15,3:1","15,3:1","15,3:1","15,3:1","15,3:1"]
["Turning circle (Curb to curb)","11,8 m","11,8 m","11,8 m","11,8 m","11,8 m","11,8 m"]
["Turning circle (Wall to wall)","11,95 m","11,95 m","11,95 m","11,95 m","11,95 m","11,95 m"]
["Turns of steering wheel end to end",2.58,2.58,2.58,2.58,2.58,2.58]
["Braking system","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)","Antilock Braking System (ABS) with Electronic Brake Distribution (EBD) and Electronic Brake Assistance (EBA)"]
["Brake disc diameter (front ventilated)","300 mm / 320 mm","300 mm / 320 mm","300 mm / 320 mm","300 mm / 320 mm","300 mm / 320 mm","300 mm / 320 mm"]
["Brake disc diameter (rear solid)","280 mm","280 mm","280 mm","280 mm","280 mm","280 mm"]
["Brake disc thickness (front)","25 mm","25 mm","25 mm","25 mm","25 mm","25 mm"]
["Brake disc thickness (rear)","11 mm","11 mm","11 mm","11 mm","11 mm","11 mm"]
["Braking distance 100-0 km/h","37,6 m","37,6 m","37,6 m","37,6 m","37,6 m","37,6 m"]
[" "]
["All figures are preliminary. Volvo reserves the right to make changes in the specifications without any notice."]