{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Technical Data"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Technical Data","index":0,"n_rows":85,"n_cols":7,"rows_kept":85,"cut":false,"hidden":false,"merged":[[31,0,31,6],[34,0,34,6],[5,0,5,6],[18,0,18,6],[17,0,17,6],[30,0,30,6],[0,0,0,6],[1,0,1,6],[2,0,2,6],[4,0,4,6],[63,0,63,6],[73,0,73,6],[79,0,79,6],[35,0,35,6],[80,0,80,6],[39,0,39,6],[74,0,74,6],[83,0,83,6],[40,0,40,6],[45,0,45,6],[46,0,46,6],[50,0,50,6],[51,0,51,6],[62,0,62,6]],"flags":["formulas_cached_only"]}
["Volvo Cars of North America"]
["2014 Volvo S80"]
["Technical Data"]
[" ","S80 3.2","S80 3.2 Premier Plus","S80 3.2 Platinum","S80 T6 AWD","S80 T6 AWD Premier Plus","S80 T6 AWD Platinum"]
[" "]
["Engine"]
["3.2 Liter, inline 6-cylinder, double overhead cam, 24-valve","STD","STD","STD","-","-","-"]
["3.0 Liter, inline 6-cylinder, double overhead cam, 24-valve twin-scroll turbo with intercooler","-","-","-","STD","STD","STD"]
["Compression ratio","10.8:11","10.8:11","10.8:11","9.3:1","9.3:1","9.3:1"]
["Configuration","Transverse/FWD","Transverse/FWD","Transverse/FWD","Transverse/AWD","Transverse/AWD","Transverse/AWD"]
["Displacement","3,192 cc","3,192 cc","3,192 cc","2,953 cc","2,953 cc","2,953 cc"]
["Bore x stroke","84.0 mm x 96.0 mm","84.0 mm x 96.0 mm","84.0 mm x 96.0 mm","82.0 mm x 93.2 mm","82.0 mm x 93.2 mm","82.0 mm x 93.2 mm"]
["Horsepower (SAE net)","240 hp @ 6,400 rpm2","240 hp @ 6,400 rpm2","240 hp @ 6,400 rpm2","300 hp @ 5,600 rpm","300 hp @ 5,600 rpm","300 hp @ 5,600 rpm"]
["Torque (lb.-ft. SAE net)","236 lb.-ft. @ 3,200 rpm3","236 lb.-ft. @ 3,200 rpm3","236 lb.-ft. @ 3,200 rpm3","325 lb.-ft. @ 2,100-4,200 rpm","325 lb.-ft. @ 2,100-4,200 rpm","325 lb.-ft. @ 2,100-4,200 rpm"]
["Max engine speed","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm"]
["Fuel, recommended octane","Regular","Regular","Regular","Regular","Regular","Regular"]
["1 10,3:1 (PZEV)\n2 230 hp @ 6,500 rpm (PZEV)\n3 221 lb.-ft. @ 3,300 rpm (PZEV)"," "," "," "," "," "," "]
[" "]
["Transmission"]
["Six-speed \"Geartronic\" driver-adaptive automatic","STD","STD","STD","STD1","STD1","STD1"]
["First gear",4.148,4.148,4.148,4.148,4.148,4.148]
["Second gear",2.37,2.37,2.37,2.37,2.37,2.37]
["Third gear",1.556,1.556,1.556,1.556,1.556,1.556]
["Fourth gear",1.155,1.155,1.155,1.155,1.155,1.155]
["Fifth gear",0.859,0.859,0.859,0.859,0.859,0.859]
["Sixth gear",0.686,0.686,0.686,0.686,0.686,0.686]
["Reverse gear",3.394,3.394,3.394,3.394,3.394,3.394]
["Final drive ratio","3.33:1","3.33:1","3.33:1","3.33:1","3.33:1","3.33:1"]
["Electronically controlled all-wheel drive with Instant Traction","-","-","-","STD","STD","STD"]
["1               With Sport Mode"," "," "," ","STD","STD","STD"]
[" "]
["Brakes"]
["4-channel Anti-lock Braking System (ABS) with Hydraulic Brake Assist (HBA), Optimized Hydraulic Brakes (OHB), Ready Alert Brakes (RAB) and Fading Brake Support (FBS)","STD","STD","STD","STD","STD","STD"]
["Disc diameter, front/rear","11.8/11.9 in.","11.8/11.9 in.","11.8/11.9 in.","11.8/11.9 in.","11.8/11.9 in.","11.8/11.9 in."]
[" "]
["Suspension"]
["Front suspension: MacPherson strut, with asymmetrically-mounted coil springs, hydraulic shock absorbers, stabilizer bar","STD","STD","STD","STD","STD","STD"]
["Rear suspension: Multilink independent suspension with coil springs, hydraulic shock absorbers, stabilizer bar, cast aluminum subframe","STD","STD","STD","STD","STD","STD"]
["Lowered Sport Chassis with firmer springs, retuned shocks, firmer stabilizer bars, lower ride height","-","-","-","OPT","OPT","OPT"]
[" "]
["Steering"]
["Power assisted, rack and pinion steering","STD","STD","STD","STD","STD","STD"]
["Turns, lock to lock",2.6,2.6,2.6,2.6,2.6,2.6]
["Turning circle, curb to curb","36.7 ft.","36.7 ft.","36.7 ft.","40.0 ft.","40.0 ft.","40.0 ft."]
["Steering ratio","16.0:1","16.0:1","16.0:1","16.0:1","16.0:1","16.0:1"]
[" "]
["Wheels and Tires"]
["7.0\" x 17\" - \"REX\" alloy wheels with 225/50-R17 tires","STD","STD","STD","-","-","-"]
["8.0\" x 18\" - \"Magni\" alloy wheels with 245/40-R18 tires","OPT","OPT","OPT","STD","STD","STD"]
["8.0\" x 18\" - \"Ymir\" forged alloy wheels with 245/40-R18 tires","-","-","-","PKG","PKG","PKG"]
[" "]
["Exterior Dimensions and Weights"]
["Curb weight","3,761 lbs.","3,761 lbs.","3,761 lbs.","4,053 lbs.","4,053 lbs.","4,053 lbs."]
["GVWR (Gross Vehicle Weight Ratings)","4,820 lbs.","4,820 lbs.","4,820 lbs.","5,020 lbs.","5,020 lbs.","5,020 lbs."]
["Fuel tank capacity","18.5 US gallons","18.5 US gallons","18.5 US gallons","18.5 US gallons","18.5 US gallons","18.5 US gallons"]
["Height","58.8 in.","58.8 in.","58.8 in.","58.8 in.","58.8 in.","58.8 in."]
["Length","191.1 in.","191.1 in.","191.1 in.","191.1 in.","191.1 in.","191.1 in."]
["Towing capacity","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs."]
["Track, front","62.1 in.","62.1 in.","62.1 in.","62.1 in.","62.1 in.","62.1 in."]
["Track, rear","62.0 in.","62.0 in.","62.0 in.","62.0 in.","62.0 in.","62.0 in."]
["Wheelbase","111.6 in.","111.6 in.","111.6 in.","111.6 in.","111.6 in.","111.6 in."]
["Width","73.3 in.","73.3 in.","73.3 in.","73.3 in.","73.3 in.","73.3 in."]
[" "]
["Interior Dimensions"]
["Headroom, front","37.8 in.","37.8 in.","37.8 in.","37.8 in.","37.8 in.","37.8 in."]
["Headroom, rear","38.3 in.","38.3 in.","38.3 in.","38.3 in.","38.3 in.","38.3 in."]
["Hiproom, front","54.8 in.","54.8 in.","54.8 in.","54.8 in.","54.8 in.","54.8 in."]
["Hiproom, rear","54.7 in.","54.7 in.","54.7 in.","54.7 in.","54.7 in.","54.7 in."]
["Legroom, front","41.9 in.","41.9 in.","41.9 in.","41.9 in.","41.9 in.","41.9 in."]
["Legroom, rear","35.0 in.","35.0 in.","35.0 in.","35.0 in.","35.0 in.","35.0 in."]
["Shoulder room, front","57.4 in.","57.4 in.","57.4 in.","57.4 in.","57.4 in.","57.4 in."]
["Shoulder room, rear","56.3 in.","56.3 in.","56.3 in.","56.3 in.","56.3 in.","56.3 in."]
["Trunk capacity","14.9 cu. ft.","14.9 cu. ft.","14.9 cu. ft.","14.9 cu. ft.","14.9 cu. ft.","14.9 cu. ft."]
[" "]
["Performance"]
["Top speed (electronically limited)","130 mph","130 mph","130 mph","155 mph","155 mph","155 mph"]
["Acceleration (0-60 mph) automatic transmission - estimated","7.4 sec.1","7.4 sec.1","7.4 sec.1","6.0 sec.","6.0 sec.","6.0 sec."]
["Stopping distance (from 62 mph)","134.5 ft.","134.5 ft.","134.5 ft.","134.5 ft.","134.5 ft.","134.5 ft."]
["1               7.9 PZEV"," "," "," "," "," "," "]
[" "]
["Fuel Economy"]
["Automatic transmission, city (estimated)","19 mpg","19 mpg","19 mpg","18 mpg","18 mpg","18 mpg"]
["Automatic transmission, highway (estimated)","28 mpg","28 mpg","28 mpg","25 mpg","25 mpg","25 mpg"]
[" "]
["Volvo Cars of North America, LLC reserve the right to make changes at any time, without notice, to color, specifications, accessories, materials and models."]