{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Technical Data"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Technical Data","index":0,"n_rows":92,"n_cols":8,"rows_kept":92,"cut":false,"hidden":false,"merged":[[5,0,5,7],[20,0,20,7],[0,0,0,7],[1,0,1,7],[2,0,2,7],[4,0,4,7],[80,0,80,7],[85,0,85,7],[38,0,38,7],[39,0,39,7],[21,0,21,7],[34,0,34,7],[35,0,35,7],[66,0,66,7],[42,0,42,7],[90,0,90,7],[43,0,43,7],[48,0,48,7],[49,0,49,7],[52,0,52,7],[53,0,53,7],[65,0,65,7],[86,0,86,7],[79,0,79,7]],"flags":["formulas_cached_only"]}
["Volvo Cars of North America"]
["2014 Volvo XC70 Cross Country"]
["Technical Data"]
[" ","XC70 3.2","XC70 3.2 Premier","XC70 3.2 Premier Plus","XC70 3.2 Platinum","XC70 T6 AWD","XC70 T6 AWD Premier Plus","XC70 T6 AWD Platinum"]
[" "]
["Engine"]
["3.2 Liter, inline 6-cylinder, double overhead cam, 24-valve","STD","STD","STD","STD","-","-","-"]
["3.0 Liter, inline 6-cylinder, double overhead cam, 24-valve twin-scroll turbo with intercooler","-","-","-","-","STD","STD","STD"]
["Compression ratio","10.8 : 11","10.8 : 11","10.8 : 11","10.8 : 11","9.3 : 1","9.3 : 1","9.3 : 1"]
["Configuration","Transverse/FWD / AWD (Optional)","Transverse/FWD / AWD (Optional)","Transverse/FWD / AWD (Optional)","Transverse/FWD / AWD (Optional)","Transverse/AWD","Transverse/AWD","Transverse/AWD"]
["Displacement","3,192 cc","3,192 cc","3,192 cc","3,192 cc","2,953 cc","2,953 cc","2,953 cc"]
["Bore x stroke","84.0 x 96.0 mm","84.0 x 96.0 mm","84.0 x 96.0 mm","84.0 x 96.0 mm","82.0 x 93.2 mm","82.0 x 93.2 mm","82.0 x 93.2 mm"]
["Horsepower (SAE net)","240 @ 6,400 rpm2","240 @ 6,400 rpm2","240 @ 6,400 rpm2","240 @ 6,400 rpm2","300 @ 5,600 rpm","300 @ 5,600 rpm","300 @ 5,600 rpm"]
["Torque (lb.-ft. SAE net)","236 @ 3,200 rpm3","236 @ 3,200 rpm3","236 @ 3,200 rpm3","236 @ 3,200 rpm3","325 @ 2,100-4,200 rpm","325 @ 2,100-4,200 rpm","325 @ 2,100-4,200 rpm"]
["Max engine speed","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm","6,500 rpm"]
["Fuel, rec. octane","Regular","Regular","Regular","Regular","Regular","Regular","Regular"]
["1               10.3:1 for PZEV engine"," "," "," "," "," "," "," "]
["2               230 hp @ 6,500 rpm for PZEV engine"," "," "," "," "," "," "," "]
["3               221 @ 3,300 rpm for PZEV engine"]
[null," "," "," "," "," "," "," "]
[" "]
["Transmission"]
["Six-speed \"Geartronic\" driver-adaptive automatic","STD","STD","STD","STD","STD1","STD1","STD1"]
["Gear ratios"," "," "," "," "," "," "," "]
["First gear","4.15 : 1","4.15 : 1","4.15 : 1","4.15 : 1","4.15 : 1","4.15 : 1","4.15 : 1"]
["Second gear","2.37 : 1","2.37 : 1","2.37 : 1","2.37 : 1","2.37 : 1","2.37 : 1","2.37 : 1"]
["Third gear","1.56 : 1","1.56 : 1","1.56 : 1","1.56 : 1","1.56 : 1","1.56 : 1","1.56 : 1"]
["Fourth gear","1.16 : 1","1.16 : 1","1.16 : 1","1.16 : 1","1.16 : 1","1.16 : 1","1.16 : 1"]
["Fifth gear","0.86 : 1","0.86 : 1","0.86 : 1","0.86 : 1","0.86 : 1","0.86 : 1","0.86 : 1"]
["Sixth gear","0.69 : 1","0.69 : 1","0.69 : 1","0.69 : 1","0.69 : 1","0.69 : 1","0.69 : 1"]
["Reverse gear","3.39 : 1","3.39 : 1","3.39 : 1","3.39 : 1","3.39 : 1","3.39 : 1","3.39 : 1"]
["Final drive ratio","3.75 : 1","3.75 : 1","3.75 : 1","3.75 : 1","3.46 : 1","3.46 : 1","3.46 : 1"]
["Electronically controlled all-wheel drive with Instant Traction","OPT","OPT","OPT","OPT","STD","STD","STD"]
["1               With Sport Mode"," "," "," "," "," "," "," "]
[" "]
["Brakes"]
["4-channel Anti-lock Braking System (ABS) with Hydraulic Brake Assist (HBA), Optimized Hydraulic Brakes (OHB), Ready Alert Brakes (RAB) and Fading Brake Support (FBS)","STD","STD","STD","STD","STD","STD","STD"]
["Disc diameter, front/rear","12.4 / 11.9 in.","12.4 / 11.9 in.","12.4 / 11.9 in.","12.4 / 11.9 in.","12.4 / 11.9 in.","12.4 / 11.9 in.","12.4 / 11.9 in."]
[" "]
["Suspension"]
["Front suspension: MacPherson strut, with asymmetrically-mounted coil springs, hydraulic shock absorbers, stabilizer bar","STD","STD","STD","STD","STD","STD","STD"]
["Rear suspension: Multilink independent suspension with coil springs, hydraulic shock absorbers, stabilizer bar, cast aluminum subframe","STD","STD","STD","STD","STD","STD","STD"]
[" "]
["Steering"]
["Power assisted, rack and pinion steering","STD","STD","STD","STD","STD","STD","STD"]
["Turns, lock to lock",2.8,2.8,2.8,2.8,2.8,2.8,2.8]
["Turning circle, curb to curb","37.7 ft.","37.7 ft.","37.7 ft.","37.7 ft.","37.7 ft.","37.7 ft.","37.7 ft."]
["Steering ratio","16.0 : 1","16.0 : 1","16.0 : 1","16.0 : 1","16.0 : 1","16.0 : 1","16.0 : 1"]
[" "]
["Wheels and Tires"]
["7.5\" x 17\" - \"Valder\" Alloy Wheels with 235/55-R17 Tires","STD","STD","STD","STD","-","-","-"]
["7.5\" x 18\" - \"Zephyrus\" Alloy Wheels with 235/50-R18 Tires","OPT","OPT","OPT","OPT","STD","STD","STD"]
[" "]
["Exterior Dimensions and Weights"]
["Curb weight","4,147 lbs.","4,147 lbs.","4,147 lbs.","4,147 lbs.","4,152 lbs.","4,152 lbs.","4,152 lbs."]
["GVWR (Gross Vehicle Weight Ratings)","5,258 lbs.","5,258 lbs.","5,258 lbs.","5,258 lbs.","5,300 lbs.","5,300 lbs.","5,300 lbs."]
["Front track","63.5 in.","63.5 in.","63.5 in.","63.5 in.","63.5 in.","63.5 in.","63.5 in."]
["Rear track","62.2 in.","62.2 in.","62.2 in.","62.2 in.","62.2 in.","62.2 in.","62.2 in."]
["Fuel tank capacity","18.5 U.S. gallons","18.5 U.S. gallons","18.5 U.S. gallons","18.5 U.S. gallons","18.5 U.S. gallons","18.5 U.S. gallons","18.5 U.S. gallons"]
["Ground Clearance","8.3 in.","8.3 in.","8.3 in.","8.3 in.","8.3 in.","8.3 in.","8.3 in."]
["Height","63.1 in.","63.1 in.","63.1 in.","63.1 in.","63.1 in.","63.1 in.","63.1 in."]
["Length","190.5 in.","190.5 in.","190.5 in.","190.5 in.","190.5 in.","190.5 in.","190.5 in."]
["Towing capacity","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs.","3,300 lbs."]
["Wheelbase","110.8 in.","110.8 in.","110.8 in.","110.8 in.","110.8 in.","110.8 in.","110.8 in."]
["Width","73.6 in.","73.6 in.","73.6 in.","73.6 in.","73.6 in.","73.6 in.","73.6 in."]
[" "]
["Interior Dimensions"]
["Cargo capacity (seats down)","72.1 cu. ft.","72.1 cu. ft.","72.1 cu. ft.","72.1 cu. ft.","72.1 cu. ft.","72.1 cu. ft.","72.1 cu. ft."]
["Cargo capacity (seats up)","33.3 cu. ft.","33.3 cu. ft.","33.3 cu. ft.","33.3 cu. ft.","33.3 cu. ft.","33.3 cu. ft.","33.3 cu. ft."]
["Headroom, front with sunroof","-","37.8 in.","37.8 in.","37.8 in.","37.8 in.","37.8 in.","37.8 in."]
["Headroom, front without sunroof","38.8 in.","-","-","-","-","-","-"]
["Headroom, rear with sunroof","-","38.5 in.","38.5 in.","38.5 in.","38.5 in.","38.5 in.","38.5 in."]
["Headroom, rear without sunroof","38.6 in.","-","-","-","-","-","-"]
["Hiproom, front","54.8 in.","54.8 in.","54.8 in.","54.8 in.","54.8 in.","54.8 in.","54.8 in."]
["Hiproom, rear","55.1 in.","55.1 in.","55.1 in.","55.1 in.","55.1 in.","55.1 in.","55.1 in."]
["Legroom, front","41.9 in.","41.9 in.","41.9 in.","41.9 in.","41.9 in.","41.9 in.","41.9 in."]
["Legroom, rear","34.6 in.","34.6 in.","34.6 in.","34.6 in.","34.6 in.","34.6 in.","34.6 in."]
["Shoulder room, front","57.4 in.","57.4 in.","57.4 in.","57.4 in.","57.4 in.","57.4 in.","57.4 in."]
["Shoulder room, rear","56.5 in.","56.5 in.","56.5 in.","56.5 in.","56.5 in.","56.5 in.","56.5 in."]
[" "]
["Fuel Economy"]
["Automatic transmission, FWD city (estimated)","19 mpg","19 mpg","19 mpg","19 mpg","-","-","-"]
["Automatic transmission, AWD city (estimated)","18 mpg","18 mpg","18 mpg","18 mpg","17 mpg","17 mpg","17 mpg"]
["Automatic transmission, FWD highway (estimated)","25 mpg","25 mpg","25 mpg","25 mpg","-","-","-"]
["Automatic transmission, AWD highway (estimated)","24 mpg","24 mpg","24 mpg","24 mpg","23 mpg","23 mpg","23 mpg"]
[" "]
["Performance"]
["Top speed (electronically limited)","130 mph","130 mph","130 mph","130 mph","130 mph","130 mph","130 mph"]
["Acceleration (0-60 mph) automatic transmission - estimated","8.4 sec.1","8.4 sec.1","8.4 sec.1","8.4 sec.1","6.5 sec.","6.5 sec.","6.5 sec."]
["1               8.7 PZEV"," "," "," "," "," "," "," "]
[" "]
["Volvo Cars of North America, LLC reserve the right to make changes at any time, without notice, to color, specifications, accessories, materials and models."]